**GLOSSARY**

The following terms shall have the respective meanings given below:

|  |  |
| --- | --- |
| **Abbreviation** | **Description** |
| + | Plus |
| - | Minus |
| ± | Plus or minus |
| % | Percent |
| o | Degree |
| AC | Alternating Current |
| ArchSD | Architectural Services Department |
| cm | Centimetre |
| CMH | Chinese Medicine Hospital |
| CRI | Colour rendering index |
| d10 | The diameter in which the center is Ec (maximum illumination) and the outer limit is 10% of Ec |
| d50 | The diameter in which the center is Ec and the outer limit is 50% of maximum illumination. |
| Ec | Central Illuminance |
| Ee | Irradiance |
| EMSD | Electrical and Mechanical Services Department |
| FS | Fire Services |
| HD | High Definition |
| HKSAR | Hong Kong Special Administrative Region (HKSAR) |
| Hz | Hertz |
| ICE | Independent Checking Engineer |
| IEC | International Electrotechnical Commission |
| IP | Ingress Protection |
| ISO | International Organization for Standardization |
| K | Kelvin |
| kg | Kilogram |
| m | Metre |
| mm | Millimetre |
| L1+L2 | Illumination Depth |
| LED | Light Emitting Diode |
| OT | Operating Theatre |
| PBB | Polybrominated Biphenyls |
| PBDE | Polybrominated Diphenyl Ethers |
| PCB | Printed Circuit Board |
| R9 | The score that represents how accurately a light source will reproduce strong red colour |
| Ra | General Colour Rendering Index |
| REW | Registered Electrical Workers |
| RoHS | Restriction of Hazardous Substances in Electrical and Electronic Equipment |
| VA | Volt-Ampere |
| w/m2 | Watt per square metre |