**GLOSSARY**

The following terms shall have the respective meanings given below:

|  |  |
| --- | --- |
| **Abbreviation** | **Description** |
| - | Minus |
| % | Percent |
| + | Plus |
| + | Plus or minus |
| ≤ | Smaller than or equal to |
| o C | Degree Celsius |
| A | Amperes |
| A.C. | Alternating Current |
| Amp | Ampere |
| APDs | Avalanche Photodiodes |
| APEO | Alkylphenol Ethoxylates |
| BS | British Standards |
| CFC | Chlorofluorocarbons |
| CMH | Chinese Medicine Hospital |
| CO2 | Carbon Dioxide |
| dB(A) | Decibel |
| EMSD | Electrical and Mechanical Services Department |
| HCFCs | Hydrochlorofluorocarbons |
| HKSAR | Hong Kong Special Administrative Region (HKSAR) |
| Hz | Hertz |
| IEC | International Electrotechnical Commission |
| ISO | International Organization for Standardization |
| ISM | Industrial, Scientific, and Medical |
| kg | Kilogram |
| kPa | Kilopascal |
| kW | Kilowatt |
| L | Litre |
| LED | Light Emitting Diode |
| L/h | Litre/hour |
| I/s | Litre per second |
| m | Metre |
| mbar | Millibar Pressure Unit |
| mm | Millimeter |
| MPa | Megapascal |
| nos. | Numbers |
| PBBs | Polybrominated Biphenyls |
| PBDEs | Polybrominated Diphenyl Ethers |
| Ph / V / Hz | Phase / Volts per hertz |
| RoHS | Restriction of Hazardous Substances |
| rpm | Revolutions per Minute |
| V | voltage |
| W | Watt |